How to Connect Printer in

Active Directory

By: Ruben Thomas Y. Reyes III

1.) To start off make sure that the printer is running, and you can access the settings. Under the settings there should be a network connection setting where you are able to customize a static IP address.

2.) When you have set up a static IP address, subnet mask, and default gateway for the printer you may now connect it to the ethernet. To make sure that the printer is online you must. Ping it using the command “ping “the ip address of your computer” through a computer that is on the same network. You’ll know that the printer is live and running if the packets were successfully received with the ping command.

3.) Once the printer is connected to the network. You can now customize it in windows server 2022 using the printer drivers. Usually when you install the printer drivers it will give you more accessibility and customization to the printer when installed.

4.) Once you’ve installed the drivers and connect it to the server. The server will ask you if you want to share the printer click yes and the printer will share it through the network in which the computers in the same network will receive.